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REPAIR KITS FOR MODEL 507 SERIES OIL CONTROLLER

MODEL K507L & K507L-HP

RK-K507L

CONSISTS OF:

(1) RETAINING RING

(1) SCREEN

(1) VALVE SEAT, BUNA-N

(1) K507-L FLOAT ASSEMBLY

(1) CLEVIS PIN

(1) E-RING
MODEL K507L-V & K507L-V-HP

RK-K507L-V

CONSISTS OF:
(1) RETAINING RING

(1) SCREEN

(1) VALVE SEAT, VITON
(1) K507-L FLOAT ASSEMBLY

(1) CLEVIS PIN

(1) E-RING

MODEL K507L (ALL K507L’S)

MS-K507L (SWITCH KIT)
CONSISTS OF:

(1) INSULATOR BUSHING

(1) SET SCREW, SLOTTED CUP POINT, 10-32
(1) STANDOFF

(2) SETSCREW, SOCKET HEAD, 4-40 X 1/8”

(1) WRENCH, .050” ALLEN
MODEL 507L & 507L-HP:

RK-507L

CONSISTS OF:

(1) RETAINER RING

(1) COTTER PIN 

(1) CLEVIS PIN 

(1) 507-L FLOAT ASSEMBLY

(1) VALVE SEAT, BUNA-N

(1) SCREEN

MODEL 507L-V & 507L-V-HP:

RK-507L-V

CONSISTS OF:

(1) RETAINER RING

(1) COTTER PIN (ZP)

(1) CLEVIS PIN (ZP)

(1) 507-L FLOAT ASSEMBLY

(1) VALVE SEAT, VITON

(1) SCREEN
MODEL 507M & 507M-HP: 

RK-507M

CONSISTS OF:

(1) FLOAT ASSEMBLY

(1) SEAL, BUNA-N

(1)CLEVIS PIN

(1) COTTER PIN

(1) GASKET

(1) RETAINER RING

(1) SCREEN

MODEL 507M-V & 507M-V-HP:

RK-507M-V

CONSISTS OF:
(1) FLOAT ASSEMBLY

(1) SEAL, VITON

(1) CLEVIS PIN

(1) COTTER PIN

(1) GASKET

(1) RETAINER RING

(1) SCREEN
